**P O T A B L E W A T E R B U N K E R L O G**

**REF.** [**Health**](http://srv-glas301:82/Leisure/content/parent%20category%20topics/procedures%20and%20operations/health.htm) **> 1.0 Hygiene & Sanitation >** **[1.9 Safe Water Supplies](javascript:void(0);) AND CDC VSP MANUAL 5.2.1**

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **PORT** | |  |  | |  | |  |
| **DATE** | |  |  | |  | |  |
| **HOSES CORRECTLY RIGGED?** | |  |  | |  | |  |
| **HOSES AND SHORE LINES FLUSHED?** | |  |  | |  | |  |
| **MICROBIOLOGIC REPORT RECEIVED?** | |  |  | |  | |  |
| **SHORE SAMPLE CERTIFICATE RESULT** | | **CHL** |  | | **pH** | |  |
| **SAMPLE SHORESIDE PRE-TEST RESULT BEFORE COMMENCEMENT** | | **CHL** |  | | **pH** | |  |
| **TIME COMMENCED BUNKERS** | |  |  | |  | |  |
| **CALIBRATION OF CHART RECORDER** | |  |  | |  | |  |
| **TIME RESIDUAL HALOGEN ADJUSTED TO MIN 2 PPM**  **( WITHIN 30 MINS AFTER THE START OF BUNKERING)** | | **CHL**  **MIN 2.0**  **PPM** |  | | **pH** | |  |
| **Time** |  | | | | |
| **TIME RESIDUAL HALOGEN LEVEL OF MIN 2 PPM AND PH NOT EXCEEDING 7.8 REACHED** | | **CHL**  **MIN 2.0**  **PPM** |  | | **pH MAX 7.8** | |  |
| **Time** |  | | | | |
| **HOURLY TESTS AFTER ABOVE TIME**  **IN CASE CALIBRATED CHART RECORDER IS NOT AVAILABLE** | | | | | | | |
| **TIME** |  | **CHL** |  | **pH** | |  | |
| **TIME** |  | **CHL** |  | **pH** | |  | |
| **TIME** |  | **CHL** |  | **pH** | |  | |
| **TIME** |  | **CHL** |  | **pH** | |  | |
| **TIME** |  | **CHL** |  | **pH** | |  | |
| **TIME** |  | **CHL** |  | **pH** | |  | |
| **TIME** |  | **CHL** |  | **pH** | |  | |
| **TIME** |  | **CHL** |  | **pH** | |  | |
| **TIME** |  | **CHL** |  | **pH** | |  | |
| **TIME** |  | **CHL** |  | **pH** | |  | |
| **TIME** |  | **CHL** |  | **pH** | |  | |
| **TIME** |  | **CHL** |  | **pH** | |  | |
| **TIME COMPLETE BUNKERS** | |  |  |  | |  | |
| **RESPONSIBLE OFFICER** | |  |  |  | |  | |
| **SIGNATURE** | |  |  |  | |  | |

**Free residual halogen requirement for bunkered water must be:**

**minimum 2ppm chlorine (CHL)**

**max 7.8 pH**

(Retain this Log onboard for min 12 months)