Ship:                 Period: From       To:

**Individual Hydrotherapy Pools and associated recirculation systems (or similar equipment like spa pedicure tube/throne):**

* Disinfected between each occupant / customer with an appropriate halogen-based disinfectant at min 100 ppm for 6 minutes or equivalent Concentration x Time (CT) value *under normal (non – enhanced epidemic control) sanitation. For further details see Hygiene Log PH 16 (“Normal Sanitation and Enhanced Epidemic Control Sanitation”))* and weekly
* Log maintained, as per below, for equipment: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

| Date | Time | Between each occupant | Disinfected  Pool / basin | Disinfected  associated recirculation system | Disinfectant – type, name | Concentration x Time  (CT) Value (equal to 100 ppm for 6 min) | | Responsible person, signed: |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Concentra-tion ppm | Time |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |

Spa Manager:       Hotel Manager:

*Maintain this log onboard for at least 12 months*