Ship:                 Month:       Year:

* A minimum of four potable water samples per month shall be collected and analysed for the presence of E-coli (Escherichia coli):
  + Analysis shall be made using an approved test kit.
  + Samples shall be collected randomly from locations forward, aft, upper and lower decks of the vessel
    - *microbiological samples from ice machines and potable water storage tanks do not count toward the monthly routine distribution system monitoring*
  + Sample sites should be changed each month in order to obtain a good representation of the potable water distribution system
  + **Follow up sampling must be conducted for each positive test result**

| Date | Sample point location:  Fwd or aft;  specify | Sample point location:  upper or lower deck; specify | Different from last month Y/N | E-Coli test -positive or negative | Corrective Action if test positive | Responsible person, signed: |
| --- | --- | --- | --- | --- | --- | --- |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |

Doctor:       Staff Captain:

*Maintain this log onboard for at least 12 months*