Ship:                 Year:

* Back-Flow Preventers (**BFP**) requiring testing (for example ‘reduced pressure backflow preventers’ and ‘pressure vacuum breakers’) shall be tested and inspected with a test kit after installation and at least annually

| BFP location | BFP type | Date | Valve A | | | Valve B | | | Remarks | Resp. person, signed: |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Pressure 1 | Pressure 2 | Difference | Pressure 1 | Pressure 2 | Difference |
|  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |

* Test results showing the pressure differences on both sides of the valves shall be maintained for each device

*add additional pages if necessary for the list above:*      *pages added)*

Date:       Hotel Engineer:       Chief Engineer:

(*Maintain this log onboard for at least 12 months)*