Ship:                 Quarter:       Year:

* Shower heads and faucets must be dismantled (as possible incl. aerator and mesh), cleaned with an acidic bathroom cleaner using a nylon brush, rinsed and disinfected every 6 months. DISINFECTION must be accomplished with an appropriate halogen-based disinfectant at 100 ppm for 10 minutes or equivalent Concentration x Time value

| Cabin No. /Location | Date | Type: showerhead or Faucet | Position | Crewmember name/sign | Supervisor Name/sign |
| --- | --- | --- | --- | --- | --- |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |

Housekeeper:       Hotel Manager:

*Maintain this log onboard for at least 12 months*