# QUARTERLY SAFETY DEVICES REPORT

**VESSEL :** \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ **DATE :** \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | **ORIGINAL**  **SETTING** | **DATE TESTED** | | | | | | | | **REMARKS** |
| **MAIN ENGINE** |  | 1 | | 2 | | 3 | | 4 | |  |
| LUB OIL ALARM |  |  | |  | |  | |  | |  |
| LUB OIL TRIP |  |  | |  | |  | |  | |  |
| JACKET CW ALARM |  |  | |  | |  | |  | |  |
| JACKET CW TRIP |  |  | |  | |  | |  | |  |
| PISTON COOLING ALARM |  |  | |  | |  | |  | |  |
| PISTON COOLING TRIP |  |  | |  | |  | |  | |  |
| OVERSPEED |  |  | |  | |  | |  | |  |
| ME CYL OIL NON FLOW |  |  | |  | |  | |  | |  |
| FUEL LEAKAGE ALARM |  |  | |  | |  | |  | |  |
| **BOILER** (**check monthly**!) |  |  | |  | |  | |  | |  |
| LOW LEVEL ALARM |  |  | |  | |  | |  | |  |
| LOW LEVEL TRIP |  |  | |  | |  | |  | |  |
| HI LEVEL ALARM |  |  | |  | |  | |  | |  |
| FLAME FAILURE ALARM |  |  | |  | |  | |  | |  |
| FLAME FAILURE TRIP |  |  | |  | |  | |  | |  |
| OVERSPEED |  |  | |  | |  | |  | |  |
| OTHER SAFETY DEVICES (specify: ) |  |  | |  | |  | |  | |  |
| **DIESEL GENERATOR** |  | 1 | 2 | 3 | 4 | 5 | 6 | 7 | EM |  |
| LUB OIL ALARM |  |  |  |  |  |  |  |  |  |  |
| LUB OIL TRIP |  |  |  |  |  |  |  |  |  |  |
| COOLING WATER ALARM |  |  |  |  |  |  |  |  |  |  |
| COOLING WATER TRIP |  |  |  |  |  |  |  |  |  |  |
| OVERSPEED |  |  |  |  |  |  |  |  |  |  |
| FUEL LEAKAGE ALARM |  |  |  |  |  |  |  |  |  |  |
| **TURBO GENERATOR** |  |  |  |  |  |  |  |  |  |  |
| LUB OIL ALARM |  |  |  |  |  |  |  |  |  |  |
| LUB OIL TRIP |  |  |  |  |  |  |  |  |  |  |
| OVERSPEED |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |
| **BILGE ALARMS** |  |  |  |  |  |  |  |  |  |  |
| **NOTE: All cut out and alarms have to be verified once a quarter** | | | | | | | | | | |

Master \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Chief Engineer \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_