Ship:                 Period: From       To:

* At least once a month the ship’s potable water hoses and stand pipes must be sanitized as follows
  + - Flush the hose thoroughly with potable water and then drain hose.
    - Raise both ends of the hose, fill with disinfecting solution containing 100-ppm chlorine, close ends, and allow to stand for one hour.
    - Flush thoroughly with potable water before attaching at filling line.
    - Standpipes must be cleaned and disinfected with 100-ppm chlorine solution.

| Date | Time (start and stop) | Bunker Station | Hoses | Stand Pipes | Remarks | Responsible person, signed: |
| --- | --- | --- | --- | --- | --- | --- |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |

Staff Captain:

*Maintain this log onboard for at least 12 months*